|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No.  | Description/Scope | QTY | Unit price  | Total price | Delivery Period  |
|  | Gas turbine model PG6111FA+e-50HzConfiguration: DLN with bleed heating manufacturer: General Electric, France  |  |  |  |  |
| 1 | Seal stationary -oil bearing 1 GE P/N: 185D3516P001 | 1 unit |  |  |  |
| 2 | 6FA seal assembly stationary oil-bearing 1 GE P/N: 223C2 625G001 | 1 unit |  |  |  |
| 3 | 6FA seal stationary oil-bearing 1 GE P/N: 223C2626G001 | 1 unit |  |  |  |
| 4 | 6FA seal assembly stationary oil-bearing No 1 GE P/N: 223C2624G001 | 1 unit |  |  |  |
| 5 | Seal stationary – air bearing 1GE P/N: 185D3525P001 | 1 unit |  |  |  |
| 6 | Air deflector (bearing 1)GE P/N: 223C2623P001 | 1 unit |  |  |  |
| 7 | Pin, lockingGE P/N: 351A1611P001 | 1 unit |  |  |  |
| 8 | Pin, lockingGE P/N: 351A1611P002 | 1 unit |  |  |  |
| 9 | Pin, lockingGE P/N: 351A1611P003 | 1 unit |  |  |  |
| 10 | Shim, thrust bearing -AFTGE P/N: 320B7708P002 | 1 unit |  |  |  |
| 11 | Seal, stationary oil bearing no 2GE P/N: 223DC2638G001 | 1 unit |  |  |  |
| 12 | Seal, stationary oil bearing 2GE P/N: 185D3529G001 | 1 unit |  |  |  |
| 13 | Alloy steel 12 PT screw GE P/N: N733AP29016 | 32 units |  |  |  |
| 14 | Bolt 12 PTGE P/N: N733AP25040 | 2 units |  |  |  |
| Subtotal  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No.  | Description/Scope | QTY | Unit price  | Total price | Delivery Period  |
| 15 | Pin dowel, 0.375x2.00(L)GE P/N: 158A5457P004 | 8 units |  |  |  |
| 16 | 6FA rack gearGE P/N: 320B7710P002 | 4 units |  |  |  |
| 17 | Bolt hex hd-alloy steelGE P/N: N14P25032 | 32 units |  |  |  |
| 18 | Shim . 008GE P/N: 298A8537P002 | 15 units |  |  |  |
| 19 | Shim.006GE P/N: 298A8537P003 | 15 units |  |  |  |
| 20 | Shim. 010 GE P/N: 298A8537P001 | 15 units |  |  |  |
| 21 | Shim. 004GE P/N: 298A8537P004 | 15 units |  |  |  |
| 22 | Set screw, alloy steelGE P/N: N173P2308 | 64 units |  |  |  |
| 23 | Gear, IGV-MODGE P/N: 226D1414G001 | 64 units |  |  |  |
| 24 | Spring washerGE P/N: 158A7887P001 | 64 units |  |  |  |
| 25 | BushingGE P/N: 158A7888P002 | 1 unit |  |  |  |
| 26 | Washer, thrust GE P/N: 352A6633P003 | 64 units |  |  |  |
| 27 | TubingGE P/N: 372A2190P001 | 64 units |  |  |  |
| 28 | Grooved straight pinGE P/N: N512P2512B | 64 units |  |  |  |
| 29 | BushingGE P/N: 339A9913P001 | 64 units |  |  |  |
| 30 | Flexible air hose, 2 inchGE P/N: 381A62429P002 | 4 units |  |  |  |
| 31 | Expansion joint, 4 inchGE P/N: 91449954P002 | 4 units |  |  |  |
| 32 | CHECK VALCE, 1 inchGE P/N: 113A6789P002 | 6 units |  |  |  |
| Subtotal  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No.  | Description/Scope | QTY | Unit price  | Total price | Delivery Period  |
| 33 | Copper crush gasketGE P/N: 107T5134P001 | 6 units |  |  |  |
| 34 | 6FA 03 load coupling bolting tooling hardwareGE P/N: 381A6850P001This kit included:1 bolt coupling between GT to LC -27 units2 bolts coupling between LC to GB – 27 units3 bolts coupling between LGB to GEN – 18 units | 1 set |  |  |  |
| 35 | ChockGE P/N: 323B6225P001 | 4 units |  |  |  |
| 36 | Balance weight GE P/N: 0132V996P0001 | 6 units |  |  |  |
| 37 | Balance weightGE P/N: 0699L984G0001This group contains:142A7993P0001-balance weight (3.00 OZ nom) – qty: 2 units 142 A7993P0002-balance weight (3.50 OZ nom) qty: 2 units142A7993p0003-balance weight (4.00OZ nom) -qty: 6 units142A7993P0004-balance weight ( 4.50 OZ nom) – qty: 6 units0132V996P0001- balance weight -qty: 6 unitsN70P02908- screw, set- 16 unitsN70P02508-screw, set-8 units | 1 set |  |  |  |
| 38 | Edge sealGE P/N: 313A7323P0001 | 22 ft |  |  |  |
| 39 | Positioning plateGE P/N: 235C3256G0001 | 2 units |  |  |  |
| 40 | Breather capGE P/N: 323B5821P0002 | 2 units |  |  |  |
| 41 | Flexible hose braided SSTGE P/N: 03140J87P0011 | 2 units |  |  |  |
| Subtotal: |  |